Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package peak.can.basic

Interface Summary
IRcvEventProcessor | This interface is implemented by classes which need to process the CAN Receive-Event.

Class Summary
PCANBasic | This is the main class for using the PCANBasic API with your java applications.
RcvEventDispatcher | This class is a gateway between the PCAN Light JNI and the application to dispatch the CAN Receive-Event.
TPCANMsg | Defines a CAN message.
TPCANTimestamp | Defines the point of time at which a CAN message was received.

Enum Summary
TPCANBaudrate | Baud rate codes = BTR0/BTR1 register values for the CAN controller.
TPCANDevice | Represents a PCAN device
TPCANHandle | Represents a PCAN-hardware channel handle.
TPCANMode | Represents a PCAN filter mode.
TPCANParameter | Parameter definition.
TPCANParameterValue | Parameter values definition
TPCANStatus | Represent the PCAN error and status codes
TPCANType | Represents a PCAN device

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES