A C D F G H I M P R S T U V W

## S

setCanFd(boolean) - Method in class peak.can.ChannelItem
setCounter(int) - Method in class peak.can.TableDataRow
  Sets number of times the CAN Message was readed
setData(byte[], byte) - Method in class peak.can.basic.TPCANMsg
  Sets the data and length of this message.
setData(byte[], byte) - Method in class peak.can.basic.TPCANMsgFD
  Sets the data and length of this message.
setDlc(byte) - Method in class peak.can.basic.TPCANMsgFD
  Sets the data length code of this message.
setHandle(TPCANHandle) - Method in class peak.can.ChannelItem
  Sets the PCAN Handle
setID(int) - Method in class peak.can.basic.TPCANMsg
  Sets the id of this message.
setID(int) - Method in class peak.can.basic.TPCANMsgFD
  Sets the id of this message.
setLength(byte) - Method in class peak.can.basic.TPCANMsg
  Sets the length of this message.
setListener(IRcvEventProcessor) - Static method in class peak.can.basic.RcvEventDispatcher
  Sets the Receive-Event processor
setMessage(TPCANMsg) - Method in class peak.can.TableDataRow
  Sets wrapped TPCANMsg
setMessage(TPCANMsgFD) - Method in class peak.can.TableDataRow
  Sets wrapped TPCANMsgFD
setMicros(short) - Method in class peak.can.basic.TPCANTimestamp
  Sets microseconds
setMillis(int) - Method in class peak.can.basic.TPCANTimestamp
  Sets milliseconds
setMillis_overflow(short) - Method in class peak.can.basic.TPCANTimestamp
  Sets milliseconds overflow
SetRcvEvent(TPCANHandle) - Method in class peak.can.basic.PCANBasic
  Sets the handle of the Receive-Event for the Channel. static method peak.can.basic.RcvEventDispatcher.dispatchRcvEvent is used to notify each Receive-Event
setRcvTime(TPCANTimestamp) - Method in class peak.can.TableDataRow
  Sets wrapped TPCANTimestamp
setRcvTime(TPCANTimestampFD) - Method in class peak.can.TableDataRow
  Sets wrapped TPCANTimestamp
setReadTimeStamp(Boolean) - Method in class peak.can.CANReadThread
setSendInterval(int) - Method in class peak.can.CANSendThread
setType(byte) - Method in class peak.can.basic.TPCANMsg
  Sets the type of this message.
setType(EnumSet<TPCANMessageType>) - Method in class peak.can.basic.TPCANMsg
  Sets the type of this message.
setType(EnumSet<TPCANMessageType>) - Method in class peak.can.basic.TPCANMsgFD
  Sets the type of this message.
setType(byte) - Method in class peak.can.basic.TPCANMsgFD
  Sets the type of this message.
setType(TPCANType) - Method in class peak.can.ChannelItem
  Sets the PCAN Hardware Type (for Non-PNP devices only)
SetValue(TPCANHandle, TPCANParameter, Object, int) - Method in class peak.can.basic.PCANBasic
  Configures or sets a PCAN Channel value Parameters can be present or not according with the kind of Hardware (PCAN Channel) being used.
setValue(int) - Method in enum peak.can.basic.TPCANBaudrate
  Sets the user-defined value
setValue(String) - Method in class peak.can.basic.TPCANBitrateFD
setValue(long) - Method in class peak.can.basic.TPCANTimestampFD
setValue(int) - Method in class peak.can.MutableInteger
  Sets integer value
setWorking(boolean) - Method in class peak.can.ChannelItem
  Sets PCAN Handle state

A C D F G H I M P R S T U V W