# Uses of Package
peak.can.basic

- Packages that use peak.can.basic
  Package | Description
  --- | ---
  peak.can |
  peak.can.basic |

- Classes in peak.can.basic used by peak.can
  Class and Description
  IRcvEventProcessor This interface is implemented by classes which need to process the CAN Receive-Event.
  PCANBasic This is the main class for using the PCANBasic API with your java applications.
  TPCANHandle Represents a PCAN-hardware channel handle.
  TPCANMsg Defines a CAN message.
  TPCANMsgFD Defines a CAN FD message.
  TPCANTimestamp Defines the point of time at which a CAN message was received.
  TPCANTimestampFD Defines the point of time at which a CAN message was received.
  TPCANType Represents a PCAN device

- Classes in peak.can.basic used by peak.can.basic
  Class and Description
  IRcvEventProcessor This interface is implemented by classes which need to process the CAN Receive-Event.
  TPCANBaudrate Baud rate codes = BTR0/BTR1 register values for the CAN controller.
  TPCANBitrateFD Baud rate codes = BTR0/BTR1 register values for the CAN controller.
  TPCANBitrateFDValue Baud rate codes = BTR0/BTR1 register values for the CAN controller.
  TPCANDevice Represents a PCAN device
  TPCANHandle Represents a PCAN-hardware channel handle.
  TPCANMessageType Represents the type of a PCAN message
  TPCANMode Represents a PCAN filter mode.
  TPCANMsg Defines a CAN message.
  TPCANMsgFD Defines a CAN FD message.
  TPCANParameter Parameter definition.
  TPCANParameterValue Parameter values definition
  TPCANStatus Represent the PCAN error and status codes
  TPCANTimestamp Defines the point of time at which a CAN message was received.
  TPCANTimestampFD Defines the point of time at which a CAN message was received.
  TPCANType Represents a PCAN device