# Package peak.can.basic

- Interface Summary
  Interface | Description
  --- | ---
  IRcvEventProcessor | This interface is implemented by classes which need to process the CAN Receive-Event.

- Class Summary
  Class | Description
  --- | ---
  PCANBasic | This is the main class for using the PCANBasic API with your java applications.
  RcvEventDispatcher | This class is a gateway between the PCAN Light JNI and the application to dispatch the CAN Receive-Event.
  TPCANBitrateFD | Baud rate codes = BTR0/BTR1 register values for the CAN controller.
  TPCANMsg | Defines a CAN message.
  TPCANMsgFD | Defines a CAN FD message.
  TPCANTimestamp | Defines the point of time at which a CAN message was received.
  TPCANTimestampFD | Defines the point of time at which a CAN message was received.

- Enum Summary
  Enum | Description
  --- | ---
  TPCANBaudrate | Baud rate codes = BTR0/BTR1 register values for the CAN controller.
  TPCANBitrateFDValue | Baud rate codes = BTR0/BTR1 register values for the CAN controller.
  TPCANDevice | Represents a PCAN device
  TPCANHandle | Represents a PCAN-hardware channel handle.
  TPCANMessageType | Represents the type of a PCAN message
  TPCANMode | Represents a PCAN filter mode.
  TPCANParameter | Parameter definition.
  TPCANParameterValue | Parameter values definition
  TPCANStatus | Represent the PCAN error and status codes
  TPCANType | Represents a PCAN device