## Uses of Class
peak.can.basic.TPCANBitrateFD

- Packages that use TPCANBitrateFD
  Package | Description
  --- | ---
  peak.can.basic |

- - ### Uses of TPCANBitrateFD in peak.can.basic

    Methods in peak.can.basic with parameters of type TPCANBitrateFD
    Modifier and Type | Method and Description
    --- | ---
    `TPCANStatus` | PCANBasic.`InitializeFD(TPCANHandle Channel, TPCANBitrateFD BitrateFD)` Initializes a FD capable PCAN Channel See PCAN_BR_* values Bitrate string must follow the following construction rules: - parameters and values must be separated by '=' - Couples of Parameter/value must be separated by ',' - Following Parameter must be filled out: f_clock, data_brp, data_sjw, data_tseg1, data_tseg2, nom_brp, nom_sjw, nom_tseg1, nom_tseg2. - Following Parameters are optional (not used yet): data_ssp_offset, nom_samp Example: f_clock_mhz=80, nom_brp=1, nom_tset1=63, nom_tseg2=16, nom_sjw=7, data_brp=4, data_tset1=12, data_tseg2=7, data_sjw=1