Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
peak.can.basic.TPCANHandle

Packages that use TPCANHandle
peak.can |
peak.can.basic |

Uses of TPCANHandle in peak.can

Fields in peak.can declared as TPCANHandle
`protected TPCANHandle` | `ChannelItem.handle`

Methods in peak.can that return TPCANHandle
`TPCANHandle` | `ChannelItem.getHandle()` Gets the PCAN Handle

Methods in peak.can with parameters of type TPCANHandle
`void` | `CANReadThread.callAPIFunctionRead(TPCANHandle handle)` Calls the PCANBasic Read Function according the readTimeStamp parameter
`void` | `CANReadThread.processRcvEvent(TPCANHandle channel)`
`void` | `ChannelItem.setHandle(TPCANHandle handle)` Sets the PCAN Handle

Constructors in peak.can with parameters of type TPCANHandle
`ChannelItem(TPCANHandle handle)` Constructor
`ChannelItem(TPCANHandle tPCANHandle, TPCANType tPCANType)` Constructor

Uses of TPCANHandle in peak.can.basic

Methods in peak.can.basic that return TPCANHandle
`static TPCANHandle` | `TPCANHandle.valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
`static TPCANHandle[]` | `TPCANHandle.values()` Returns an array containing the constants of this enum type, in the order they are declared.

Methods in peak.can.basic with parameters of type TPCANHandle
`static boolean` | `TPCANHandle.containsSJA(TPCANHandle handle, TPCANType type)` Verify the provided TPCANHandle contains a SJA1000 controller
`static void` | `RcvEventDispatcher.dispatchRcvEvent(TPCANHandle channel)` This static public method will call from JNI to process the Receive-Event by the listener
`TPCANStatus` | `PCANBasic.FilterMessages(TPCANHandle Channel, int FromID, int ToID, TPCANMode Mode)` Configures the reception filter.
`TPCANStatus` | `PCANBasic.GetStatus(TPCANHandle Channel)` Gets the current status of a PCAN Channel
`TPCANStatus` | `PCANBasic.GetValue(TPCANHandle Channel, TPCANParameter Parameter, java.lang.Object Buffer, int BufferLength)` Retrieves a PCAN Channel value Parameters can be present or not according with the kind of Hardware (PCAN Channel) being used.
`TPCANStatus` | `PCANBasic.Initialize(TPCANHandle Channel, TPCANBaudrate Btr0Btr1, TPCANType HwType, int IOPort, short Interrupt)` Initializes a PCAN Channel
`static boolean` | `TPCANHandle.isPCANPCCardHardware(TPCANHandle handle)` Verify the provided TPCANHandle is an PC-Card Device
`static boolean` | `TPCANHandle.isPCANUSBHardware(TPCANHandle handle)` Verify the provided TPCANHandle is an USB Device
`void` | `IRcvEventProcessor.processRcvEvent(TPCANHandle channel)` This method is called by the RcvEventDispatcher to process the CAN Receive-Event by the current implementor
`TPCANStatus` | `PCANBasic.Read(TPCANHandle Channel, TPCANMsg MessageBuffer, TPCANTimestamp TimestampBuffer)` Transmits a CAN message
`TPCANStatus` | `PCANBasic.Reset(TPCANHandle Channel)` Resets the receive and transmit queues of the PCAN Channel A reset of the CAN controller is not performed.
`TPCANStatus` | `PCANBasic.ResetRcvEvent(TPCANHandle Channel)` Resets the handle of the Receive-Event for the Channel.
`TPCANStatus` | `PCANBasic.SetRcvEvent(TPCANHandle Channel)` Sets the handle of the Receive-Event for the Channel.
`TPCANStatus` | `PCANBasic.SetValue(TPCANHandle Channel, TPCANParameter Parameter, java.lang.Object Buffer, int BufferLength)` Configures or sets a PCAN Channel value Parameters can be present or not according with the kind of Hardware (PCAN Channel) being used.
`TPCANStatus` | `PCANBasic.Uninitialize(TPCANHandle Channel)` Uninitializes one or all PCAN Channels initialized by CAN_Initialize Giving the TPCANHandle value "PCAN_NONEBUS", uninitialize all initialized channels
`TPCANStatus` | `PCANBasic.Write(TPCANHandle Channel, TPCANMsg MessageBuffer)` Transmits a CAN message

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES