Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
peak.can.basic.TPCANStatus

Packages that use TPCANStatus
peak.can.basic |

Uses of TPCANStatus in peak.can.basic

Methods in peak.can.basic that return TPCANStatus
`TPCANStatus` | `PCANBasic.FilterMessages(TPCANHandle Channel, int FromID, int ToID, TPCANMode Mode)` Configures the reception filter.
`TPCANStatus` | `PCANBasic.GetErrorText(TPCANStatus Error, short Language, java.lang.StringBuffer Buffer)` Returns a descriptive text of a given TPCANStatus error code, in any desired language The current languages available for translation are: Neutral (0x00), German (0x07), English (0x09), Spanish (0x0A), Italian (0x10) and French (0x0C)
`TPCANStatus` | `PCANBasic.GetStatus(TPCANHandle Channel)` Gets the current status of a PCAN Channel
`TPCANStatus` | `PCANBasic.GetValue(TPCANHandle Channel, TPCANParameter Parameter, java.lang.Object Buffer, int BufferLength)` Retrieves a PCAN Channel value Parameters can be present or not according with the kind of Hardware (PCAN Channel) being used.
`TPCANStatus` | `PCANBasic.Initialize(TPCANHandle Channel, TPCANBaudrate Btr0Btr1, TPCANType HwType, int IOPort, short Interrupt)` Initializes a PCAN Channel
`TPCANStatus` | `PCANBasic.Read(TPCANHandle Channel, TPCANMsg MessageBuffer, TPCANTimestamp TimestampBuffer)` Transmits a CAN message
`TPCANStatus` | `PCANBasic.Reset(TPCANHandle Channel)` Resets the receive and transmit queues of the PCAN Channel A reset of the CAN controller is not performed.
`TPCANStatus` | `PCANBasic.ResetRcvEvent(TPCANHandle Channel)` Resets the handle of the Receive-Event for the Channel.
`TPCANStatus` | `PCANBasic.SetRcvEvent(TPCANHandle Channel)` Sets the handle of the Receive-Event for the Channel.
`TPCANStatus` | `PCANBasic.SetValue(TPCANHandle Channel, TPCANParameter Parameter, java.lang.Object Buffer, int BufferLength)` Configures or sets a PCAN Channel value Parameters can be present or not according with the kind of Hardware (PCAN Channel) being used.
`TPCANStatus` | `PCANBasic.Uninitialize(TPCANHandle Channel)` Uninitializes one or all PCAN Channels initialized by CAN_Initialize Giving the TPCANHandle value "PCAN_NONEBUS", uninitialize all initialized channels
`static TPCANStatus` | `TPCANStatus.valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
`static TPCANStatus[]` | `TPCANStatus.values()` Returns an array containing the constants of this enum type, in the order they are declared.
`TPCANStatus` | `PCANBasic.Write(TPCANHandle Channel, TPCANMsg MessageBuffer)` Transmits a CAN message

Methods in peak.can.basic with parameters of type TPCANStatus
`TPCANStatus` | `PCANBasic.GetErrorText(TPCANStatus Error, short Language, java.lang.StringBuffer Buffer)` Returns a descriptive text of a given TPCANStatus error code, in any desired language The current languages available for translation are: Neutral (0x00), German (0x07), English (0x09), Spanish (0x0A), Italian (0x10) and French (0x0C)

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES